
VmmDPTool update FW

Step 1. Set up the test environment

windows PC +VMM product+ monitor，After successful connection，monitor displays normal or System display setting interface can got EDID;

Step 2. Open VmmDPTool64.exe；




First, click the "Fast mode" button, which can speed up the upgrade;

Then, click the "Erase FLASH" button to erase the FW burned in the current Flash.

Step 3. Loading a new FW；

Click the "Load to FLASH" button, then select the downloaded "Panamera\_fw\_ce2L\_B1\_5.07.106\_20241107 "Open";



Step 4. Wait until the FW is successfully upgraded：

After completing the previous step, the Tool will automatically start to upgrade and the following interface will appear. The upgrade time may be affected by the ability of the computer, generally 1-2 minutes to complete;

After the upgrade is complete, reinsert the power port and Host port of the product. If the functions are normal, the upgrade succeeds.

